Gen Dem Req 01700
SECTION  16056
A & R - 16056


ELECTRICAL DEMOLITION REQUIREMENTS
Refer to the Construction Documents Directive for general editing procedures and for document coordination procedures.

See the Church Electrical Directives & Guidelines for additional information regarding the work of this Section.

UPDATE  -  1 Nov 1996

PART 1 GENERAL
 1.1
SUMMARY
A.
Includes But Not Limited To

1.
Demolition involving electrical system as described in Contract Documents.

B.
Related Sections

1.
Section 16055  -  General Electrical Requirements

2.
New and replacement work specified in appropriate specification Section.

 1.2
SCHEDULING
A.
Include on Construction Schedule specified in Section 01300 detailed sequence of individual electrical demolition operations.

B.
Coordinate with Owner for equipment and materials to be removed by Owner.

PART 2 PRODUCTS  -  Not Used

PART 3 EXECUTION
 3.1
EXAMINATION
A.
All relocations, reconnections, and removals are not necessarily indicated on Drawings.  All such work shall be included without additional cost to Owner.

 3.2
PREPARATION
A.
Disconnect equipment that is to be removed or relocated.  Carefully remove, disassemble, or dismantle as required, and store in approved location on site, existing items to be reused in completed work.

B.
Where affected by demolition or new construction, relocate, extend, or repair raceways, conductors, outlets, and apparatus to allow continued use of electrical system.  Use methods and materials as specified for new construction.

 3.3
PERFORMANCE
A.
Perform drilling, cutting, block-offs, and demolition work required for removal of necessary portions of electrical system.  Do not cut joists, beams, girders, trusses, or columns without prior written permission from Architect.

B.
Remove concealed wiring abandoned due to demolition or new construction.  Remove circuits, conduits, and conductors that are not to be re-used back to next active fixture, device, or junction box.

C.
Patch, repair, and finish surfaces affected by electrical demolition work, unless work is specifically called for under other Sections of the specifications.

 3.4
CLEANING
A.
Remove obsolete raceways, conductors, apparatus, and lighting fixtures promptly from site and dispose of legally.
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