ELC Des Guide
SECTION  16121
Supplement - 16121


HEATING CABLES
Refer to the Construction Documents Directive for general editing procedures and for document coordination procedures.

See the Church Electrical Directives & Guidelines for additional information regarding the work of this Section.

UPDATE  -  20 Oct 1997

20 Oct 97 -
Revised product specifiation format to comply with Section 01600.

PART 1 GENERAL
 1.1
SUMMARY
A.
Includes But Not Limited To

1.
Furnish and install heating cable system for rain gut​ters as described in Contract Documents.

B.
Related Sections

1.
Section 16055  -  General Electrical Requirements

PART 2 PRODUCTS
 2.1
COMPONENTS
A.
Cable

1.
Chromalox  -  TW6-CR

2.
Easy Heat  -  SMZH8-1-CBR 120 volt

3.
Raychem  -  H612 Series

4.
Thermon  -  RGC-1

B.
Temperature & Moisture Sensitive Controller

1.
Chromalox  -  GIT-2B

2.
Easy Heat  -  GIT-2B

3.
Raychem  -  GIT-2B

4.
Thermon  -  GIT-2

C.
Contactor (if required)

1.
Easy Heat  -  PC series

2.
Square 'D'  -  Class 8502

D.
Pilot Light

1.
Include plate with engraved text, >ROOF HEATING CABLE=
2.
Design Standard -

a.
Pass & Seymour 2151 Red

 2.2
ACCEPTABLE MANUFACTURERS
A.
Chromalox, Murfreesboro, TN  (615) 848-2560

B.
Easy Heat, New Carlisle, IN  (800) 537-4732

C.
Raychem Corporation, Menlo Park, CA  (800) 542-8936

D.
Thermon Manufacturing Co, San Marcos, TX  (800) 782-7653

E.
Equal as approved by Architect before bidding.  See Section 01600.

PART 3 EXECUTION
 3.1
INSTALLATION
A.
Install moisture probe for controller in rain gutter.

B.
Install pilot light in corridor or foyer to indicate when cables are operating.

C.
Terminate raceway on exterior of building at heat cable location with weatherproof junction box.

D.
Use only factory prepared, UL recognized splice and termination kits.
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