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SECTION  16140
Master - 16140


WIRING DEVICES
Refer to the Construction Documents Directive for general editing procedures and for document coordination procedures.

See the Church Electrical Directives & Guidelines for additional information regarding the work of this Section.

UPDATE  -  9 Jul 1997

PART 1 GENERAL
 1.1
SUMMARY
A.
Includes But Not Limited To

1.
Furnish and install wiring devices complete with plates as described in Contract Documents.

Delete paragraph 2 if no work on sound system.

2.
Furnish and install cover plates for sound system devices.

B.
Related Sections

1.
Section 16055  -  General Electrical Requirements

PART 2 PRODUCTS
 2.1
GENERAL
A.
Faces shall be nylon where available.

B.
Devices of single type shall be from same Manufacturer.

Edit Paragraph C if other or more specific color requirements are necessary.

C.
Devices are listed as Ivory.  Use Ivory devices on light colored walls and brown on dark walls.

 2.2
MANUFACTURED UNITS
A.
Switches

The 'Designer' style devices specified in this optional paragraph 1 are intended for use on new Projects.

1.
Rectangular Face Designer Style -

Delete the items listed below which are not used on this Project.

a.
Approved Manufacturers & Models -

1)
20 amp, single pole

a)
Arrow Hart  -  DEC120I

b)
Eagle  -  6621V

c)
Hubbell  -  2121I

d)
Leviton  -  5621+I

e)
Pass & Seymour  -  2621-I

2)
Two Pole -

a)
Arrow Hart  -  DEC220I

b)
Eagle  -  6622V

c)
Hubbell  -  2122I

d)
Leviton  -  5622+I

e)
Pass & Seymour  -  2622-I

3)
Three Way -

a)
Arrow Hart  -  DEC320I

b)
Eagle 6623V

c)
Hubbell  -  2123I

d)
Leviton  -  5623+I

e)
Pass & Seymour  -  2623-I

4)
Four Way -

a)
Arrow Hart  -  DEC420I

b)
Eagle  -  6624V

c)
Hubbell  -  2124I

d)
Leviton  -  5624+I

e)
Pass & Seymour  -  2624-I

5)
Pilot Switch -

a)
Eagle  -  6621-PL

b)
Hubbell  -  2121PL

c)
Leviton  -  5628-2+I

d)
Pass & Seymour  -  2629-I

6)
Lighted Toggle Switch -

a)
Single Pole -

(1)
Arrow hart  -  DEC120LI

(2)
Eagle  -  6631V

(3)
Hubbell  -  2121IL

(4)
Leviton  -  5631-2+I

(5)
Pass & Seymour  -  2625-I

b)
Three Way -

(1)
Arrow Hart  -  DEC320LI

(2)
Eagle  -  6633V

(3)
Hubbell  -  2123IL

(4)
Leviton  -  5633-2+I

(5)
Pass & Seymour  -  26266-I

Use this optional paragraph 1 specifying standard style devices where necessary on Addition/Remodel Projects to match existing device style. 

1.
Standard -

a.
Verified by UL to meet Fed Spec WS-896E.

Delete the items listed below in paragraph b which are not used on this Project.

b.
Approved Manufacturers & Models -

1)
20 amp, single pole

a)
Arrow Hart  -  1221I

b)
Eagle  -  2221V

c)
Hubbell  -  1221-I

d)
Pass & Seymour  -  20AC1-I

e)
Leviton  -  1221-2I

2)
Two Pole -

a)
Arrow Hart  -  1222I

b)
Eagle  -  2222V

c)
Hubbell  -  1222-I

d)
Pass & Seymour  -  20AC2-I

e)
Leviton  -  1222-2I

3)
Three Way -

a)
Arrow Hart  -  1223I

b)
Eagle  -  2223V

c)
Hubbell  -  1223-I

d)
Pass & Seymour  -  20AC3-I

e)
Leviton  -  1223-2I

4)
Four Way -

a)
Arrow hart  -  1224I

b)
Eagle  -  2224V

c)
Hubbell  -  1224-I

d)
Pass & Seymour  -  20AC4-I

e)
Leviton  -  1224-2I

5)
Pilot Switch -

a)
Arrow Hart  -  1991PL

b)
Eagle  -  2221-PL

c)
Hubbell  -  1221-PL

d)
Pass & Seymour  -  20AC1-RPL

e)
Leviton  -  1221-PLR

6)
Lighted Toggle Switch -

a)
Single Pole -

(1)
Arrow Hart  -  1991IL

(2)
Eagle  -  2221-LTV

(3)
Hubbell  -  1221-IL

(4)
Pass & Seymour  -  20AC1-ISL

(5)
Leviton  -  1221-LHI

b)
Three Way -

(1)
Arrow Hart  -  1993IL

(2)
Eagle  -  2223-LTV

(3)
Hubbell  -  1223-IL

(4)
Pass & Seymour  -  20AC3-ISL

(5)
Leviton  -  1223-LHC

Edit to fit Project circumstances.

2.
Timer Switches -

a.
Approved Manufacturers & Models-

1)
Exhaust Fans, Rest Rooms & Mother's Room -

a)
0-15 minute, no hold position.

b)
Intermatic FD15M

c)
Paragon SWD15M

d)
Tork A515M

2)
Exhaust Fans, Serving Area & Font -

a)
0-60 minute, no hold position.

b)
Intermatic FD60M

c)
Paragon SWD60M

d)
Tork A560M

3)
Electric Wall Heater Timer Switches -

a)
0-60 minute, no hold position, DPST.

b)
 Intermatic FF46H

Dimmer switches are only approved for the Cultural Center/Hall in conjunction with incandescent theater lighting or for Stake Center Chapels for low level incandescent lighting during satellite broadcasts.  They are not approved for Meetinghouse Chapels, Relief Society Rooms, Classrooms, Genealogical Centers, etc., or for use on fluorescent lighting.

3.
Dimmer Switches -

a.
Vertical slide control with faceplate.

b.
Preset, ON-OFF switch, 1000VA

c.
Approved Manufacturers & Models -

1)
Hubbell  -  AS101/AS1I

2)
Hunt  -  DAP-10-IV

3)
Leviton  -  81000-I

4)
Lightolier  -  MP1000-I

5)
Lutron  -  N-1003P-IV

6)
Pass & Seymour  -  91180-I

B.
Receptacles

The 'Designer' style devices specified in this optional paragraph 1 are intended for use on new Projects and additions to recent phase buildings to match existing devices.

1.
Rectangular Face Designer Style -

a.
15 amp, specification grade, back & side wired, self grounding.

b.
Approved Manufacturers & Models -

1)
Arrow Hart  -  DECB15I

2)
Eagle  -  6262V

3)
Hubbell  -  2152I

4)
Leviton  -  16252-I

5)
Pass & Seymour  -  26252-I

Use standard style devices specified in this optional paragraph 1 where necessary on Addition/Remodel Projects to match existing device style. 

1.
Standard Style -

a.
15 amp, specification grade, back and side wired, self grounding.

b.
Verified by UL to meet Fed Spec WC-596F.

c.
Approved Manufacturers & Models -

1)
Arrow Hart  -  5252I

2)
Eagle  -  5252V

3)
Hubbell  -  5252-I

4)
Leviton  -  5252-I

5)
Pass & Seymour  -  5252-I

2.
Range Receptacle -

a.
3-pole, 4 wire grounding, 125/250V, NEMA 14-50R, complete with plate.

b.
Approved Manufacturers & Models -

1)
Arrow Hart  -  5854N/S701

2)
Eagle  -  1258

3)
Hubbell  -  9450A

4)
Leviton  -  279

5)
Pass & Seymour  -  3894

3.
Ground Fault Circuit Interrupter (GFCI) -

a.
15 amp, specification grade.

b.
Approved Manufacturers & Models -

1)
Arrow Hart  -  GF5242I

2)
Eagle  -  646-2V

3)
Hubbell  -  GF5252I

4)
Leviton  -  6599-I

5)
Pass & Seymour  -  1591-I

C.
Telephone Jacks

1.
Desk type, 4 conductor, screw terminals.

a.
Approved Manufacturers & Models -

1)
Eagle  -  TWD3532V

2)
Leviton  -  40249-I

3)
Pass & Seymour  -  TE1-I

4)
Suttle  -  SE-625B-50

2.
Wall type, 4 conductor, screw terminals.

a.
Approved Manufacturers & Models -

1)
Eagle  -  TWD3521V

2)
Leviton  -  40257-I

3)
Pass & Seymour  -  WMTE14-I

4)
Suttle  -  SE-630AC4-50

D.
Plates

1.
Standard Cover Plates -

a.
Nylon or high impact resistant thermoplastic.

b.
Color shall match wiring device.

c.
Ganged switches shall have gang plates.

d.
Approved Manufacturers -

1)
Arrow hart

2)
Eagle

3)
Hubbell

4)
Leviton

5)
Pass & Seymour

2.
Weatherproof Receptacle Covers -

a.
Complete with corrosion resistant metal plate, spring lid cover, and weatherproof mats.

b.
Compatible with GFCI receptacles.

c.
Approved Manufacturers & Models -

1)
Arrow hart  -  4502, horizontal; 4501, vertical

2)
Eagle  -  1966, horizontal; 966, vertical

3)
Hubbell  -  CWP26H, horizontal; WP26, vertical

4)
Leviton  -  4990, horizontal; 4992, vertical

5)
Pass & Seymour  -  WPH26, horizontal; WP26, vertical

E.
Occupancy Sensors

1.
Ultrasonic type.

2.
Complete with sensor and combined relay/control transformer.

3.
Approved Manufacturers & Models -

a.
Honeywell -

1)
Sensor  -  EL7612A1001

2)
Relay/Transformer  -  EL7621A1002

b.
Lithonia -

1)
Sensor  -  LUS-500H

2)
Relay/Transformer  -  LUS-PCS

c.
Novitas -

1)
Sensor  -  01-083

2)
Relay/Transformer  -  13-012

d.
Tork -

1)
Sensor  -  SC20

2)
Relay/Transformer  -  TRP1

e.
Unenco -

1)
Sensor  -  C-600-R-QT1

2)
Relay/Transformer  -  211-QT1

f.
Watt Stopper -

1)
Sensor  -  W-500A

2)
Relay/Transformer  -  A120-E

PART 3 EXECUTION
 3.1
INSTALLATION
A.
Install devices flush with walls, straight, and solid to box.

B.
Label dimmer switch groupings with 1/16 inch thick laminated plastic composition material with contrasting color core.  Engraved letter shall be 1/4 inch high.
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