
SECTION  16150
Master - 16150


WIRING CONNECTIONS
Refer to the Construction Documents Directive for general editing procedures and for document coordination procedures.

See the Church Electrical Directives & Guidelines for additional information regarding the work of this Section.

UPDATE  -  20 Oct 1997

20 Oct 97 -
Revised product specification format to comply with Section 1600.

PART 1 GENERAL
 1.1
SUMMARY
A.
Includes But Not Limited To

1.
Quality of wiring connections used on Project.

B.
Related Sections

1.
Section 16055  -  General Electrical Requirements

PART 2 PRODUCTS
 2.1
COMPONENTS
A.
Standard Connectors

1.
Conductors No. 8 & Smaller  -  Steel spring wire connectors

2.
Conductors Larger Than No. 8  -  Pressure type terminal lugs

B.
Terminal blocks for tapping conductors

1.
Terminals shall be suitable for use with 75 deg C copper conductors.

2.
Acceptable Manufacturers & Models -

a.
Square D LBA363106

b.
Bussman 16323

c.
Equal as approved by Architect before bidding.  See Section 01600.

PART 3 EXECUTION  -  Not Used


END OF SECTION
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