ELC Des Guide
SECTION  16721
Master - 16721


TELEPHONE SYSTEMS
Refer to the Construction Documents Directive for general editing procedures and for document coordination procedures.

See the Church Electrical Directives & Guidelines for additional information regarding the work of this Section.

UPDATE  -  20 Oct 1997

20 Oct 97 -
Clarified specification for telephone cables.

PART 1 GENERAL
 1.1
SUMMARY
Edit SUMMARY Article as necessary to give an accurate, but brief description of the work of this Section and accurate listing of related work, especially if the scope of the work is not shown graphically on the Drawings.

A.
Includes But Not Limited To

1.
Furnish and install building telephone raceway and cable system as described in Contract Documents.

2.
Furnish and install main service raceway as described in Contract Documents and to comply with telephone company requirements.

B.
Related Sections

1.
Section 16055  -  General Electrical Requirements

2.
Section 16140  -  Telephone jacks and plates

3.
Owner  -  Furnish and install telephones

4.
Telephone Company -

a.
Furnish and install main service cable.

b.
Terminate building cables at terminal board.

PART 2 PRODUCTS
 2.1
COMPONENTS
A.
Telephone outlet box shall be single device box.

B.
Building Telephone System Cable

1.
CAT 3, 24 gauge, solid tinned copper, four twisted pairs.

2.
Meet requirements of  AT&T COMM CODE 103137063 Standard.

PART 3 EXECUTION
 3.1
INSTALLATION
Paragraph A may not be required if the Project involves an existing building.

A.
Install main service raceway as directed by telephone company.  Leave pull wire in raceway.

B.
Install raceway and cable from terminal board to each telephone outlet unless indicated otherwise on Drawings.

C.
Terminate cables at each outlet with specified modular telephone jack assembly.

D.
Leave adequate slack cable at terminal board for termination of each cable run.
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