
SECTION  16729
Master - 16729


SIGNAL BELL SYSTEMS
Refer to the Construction Documents Directive for general editing procedures and for document coordination procedures.

See the Church Electrical Directives & Guidelines for additional information regarding the work of this Section.

UPDATE  -  20 Oct 1997

20 Oct 97 -
Revised product specification format to comply with Section 01600.

PART 1 GENERAL
 1.1
SUMMARY
A.
Includes But Not Limited To

Paragraph 1 may require revision if an existing system is being extended or existing components relocated.

1.
Furnish and install signal bell system as described in Contract Documents.

B.
Related Sections

1.
Section 16055  -  General Electrical Requirements

PART 2 PRODUCTS
 2.1
COMPONENTS
The bell system is to be operated by push buttons, usually located outside the Bishop's Offices.  Timer systems are not acceptable.

A.
Interior Push Button

1.
120v, complete with plate

2.
Acceptable Manufacturers & Models -

a.
Edwards 821

b.
Equal as approved by Architect before bidding.  See Section 01600.

B.
Exterior Push Button

1.
120v, complete with plate

2.
Acceptable Manufacturers & Models -

a.
Edwards 852

b.
Equal as approved by Architect before bidding.  See Section 01600.

Use of chimes or devices other than the specified bells is not acceptable under any circumstances.

C.
Bell

1.
4 inch, 120 v, vibrating type

2.
Acceptable Manufacturers & Models -

a.
Edwards  -  340-4N5

b.
Simplex  -  2901-9066

c.
Tork  -  TA 340-4N5

d.
Equal as approved by Architect before bidding.  See Section 01600.

PART 3 EXECUTION  -  Not Used
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