E25.REV

DEVICES

NOTE: MASTER COPY DATE: JUNE, 1988.

Part 1 -	GENERAL

1)	DESCRIPTION

A.	Complete material as noted.

2)	SUBMITTALS

A.	Shop drawings:

1.	Wall switches. *

2.	Insertion receptacles. *

3.	Momentary Contact Switches. *

4.	Pilot lights. *

5.	Device plates. *

6.	Clocks.

7.	Time switches. *

8.	Surface metal raceway with devices.

Part 2 -	PRODUCTS

1)	MATERIALS

A.	Wall switches:

1.	Heavy duty, toggle, quiet type.

2.	20 amp, 120/277 volt, AC.

3.	Similar to Arrow-Hart Nos. indicated.

a.	Single pole No. 1991.

b.	Double pole No. 1992.

c.	3 way No. 1993.

d.	4 way No. 1994.

B.	Insertion receptacles:

1.	Grounded, except as noted. Meeting NEMA standards, publication WD-1-197.

2.	Similar to Arrow-Hart Nos. indicated.

3.	Duplex convenience.

a.	125 volts, 2 pole, 3 wire, grounded.

NOTE: -CHOOSE 20 AMP FOR 20 AMP BRANCH CIRCUITS AND 15 AMP FOR 15 AMP BRANCH CIRCUITS

b.	20 amp, similar to 5739S.

c.	15 amp, similar to No. 5262S.

4.	Outdoors:

a.	Duplex convenience.

b.	Weatherproof, lift-lid hinged covers. Similar to No. 4500.

5.	Clocks: single regressed receptacle, 3 wire, similar to No. 5708.

6.	Single, floor machine:

a.	20 amp, turn-to-lock action, similar to No. 6200.

b.	125 volt, 2 pole, 3 wire, grounded.

7.	Single, water cooler:

a.	20 amp, similar to No. 5361.

b.	125 volt, 2 pole, 3 wire, grounded.

8.	Special purpose:

NOTE: ADD OR DELETE AS REQUIRED.

a.	Type -----: Single, 20 amp, 250 volt, 2 pole, 3 wire, grounded, similar to No. 5861.

b.	Type ----: Single, 20 amp, 277 volt, 2 pole, 3 wire, grounded, similar to No. 7621.

c.	Type -----: Single, 20 amp, 125/250 volt, 3 pole, 4 wire, grounded, similar to No. 5759.

d.	Type -----: Single, 20 amp, 250 volt, 3 pole, 4 wire, grounded, similar to No. 5781.

e.	Type -----: Single, 30 amp, 125 volt, 2 pole, 3 wire, grounded, similar to No. 5716.

f.	Type -----: Single, 30 amp, 250 volt, 2 pole, 3 wire, grounded, similar to No. 5700.

g.	Type -----: Single, 30 amp, 277 volt, 2 pole, 3 wire, grounded, similar to No. 5795.

h.	Type -----: Single, 30 amp, 125/250 volt, 3 pole, 4 wire, grounded, similar to No. 5744.

i.	Type -----: Single, 30 amp, 250 volt, 3 pole, 4 wire, grounded, similar to No. 8430.

j.	Type -----: Single, 20 amp, turn-to-lock action, 250 volt, 2 pole, 3 wire, grounded, similar to No. 6210.

k.	Type -----: Single, 20 amp, turn-to-lock action, 277 volt, 2 pole, 3 wire, grounded, similar to No. 6220.

l.	Type -----: Single, 20 amp, turn-to-lock action, 125/250 volt, 3 pole, 4 wire, grounded, similar to No. 6400.

m.	Type -----: Single, 20 amp, turn-to-lock action, 250 volt, 3 pole, 4 wire, grounded, similar to No. 6420.

n.	Type -----: Single, 20 amp, turn-to-lock action, 120/208 volt, 4 pole, 5 wire, grounded, similar to No. 6470.

o.	Type -----: Single, 30 amp, turn-to-lock action, 125 volt, 2 pole, 3 wire, grounded, similar to No. 6330.

p.	Type -----: Single, 30 amp, turn-to-lock action, 250 volt, 2 pole, 3 wire, grounded, similar to No. 6340.

q.	Type -----: Single, 30 amp, turn-to-lock action, 277 volt, 2 pole, 3 wire,, grounded, similar to No. 6360.

r.	Type -----: Single, 30 amp, turn-to-lock action, 125/250 volt, 3 pole, 4 wire, grounded, similar to No. 6510.

s.	Type -----: Single, 30 amp, turn-to-lock action, 250 volt, 3 pole, 4 wire, grounded, similar to No. 6520.

t.	Type -----: Single, 30 amp, turn-to-lock action, 120/208 volt, 4 pole, 5 wire, grounded, similar to No. 6610.

u.	Type -----: Single, 60 amp, turn-to-lock action, 600 volt, 3 pole, 4 wire, grounded, similar to No. 26420.

v.	Type -----: Single, 60 amp, turn-to-lock action, 600 volt, 4 pole, 5 wire, grounded, similar to No. 26520.

9.	Health care facilities:

NOTE: THE N.E.C. ONLY REQUIRES PAR. (a) THRU (d) IN HAZARDOUS AND NON-HAZARDOUS ANESTHETIZING LOCATIONS, HOWEVER S AND H ALSO RECOMMENDS THEIR USE IN ICU, CCU, RECOVERY, PSYCHIATRIC, LONG TERM CARE, MATERNITY, REHAB, EMERG FOOD SERVICE, LABORATORIES, MAINTENANCE RMS, AND ABOVE 1.52M (5 FT 0 IN.) A.F.F. IN SURGERY, DELIVERY, ANESTHESIA AND INCUBATOR ROOMS

a.	Type _____: Duplex, 15 amp, 125 volts, 2 pole, 3 wire, U ground slot, similar to Hubbell No. 8200 hospital grade.

b.	Type _____: Duplex, 20 amp, 125 volts, 2 pole, 3 wire, U ground slot, similar to Hubbell No. 8300 hospital grade.

c.	Type _____: Single, 20 amp, 125 volt, 2 pole, 3 wire, U ground slot, similar to Hubbell No. 8310 hospital grade.

d.	Type _____: Single, locking type, 20 amp, 125 volts, 2 pole, 3 wire, grounded, similar to Hubbell No. 23000-HG hospital grade.

NOTE: BELOW 1.52M (5 FT 0 IN.) A.F.F. IN SURGERY, DELIVERY, ANESTHESIA AND INCUBATOR RMS AND CLASS I, GROUP C AREAS

e.	Type _____: Single, XP type, cast aluminum, polish chrome finished device plate, 20 amp, 125 volts, 2 pole, 3 wire, grounded, similar to Hubbell No. 24353.

f.	Type _____: Single, XR type, with stainless steel device plate and 8 in. x 8 in. x 4 in. wall box, 50 amp, 125 volts, 2 pole, 3 wire, grounded, similar to Hubbell No. 25505.

g.	Type _____: Single, XR type, with stainless steel device plate and 8 in. x 8 x 4 in. wall box, 60 amp, 125 volts, 2 pole, 3 wire, grounded, similar to Hubbell No. 25605.

NOTE: GROUND FAULT INTERRUPTER RECEPTACLES, SPECIFY FOR USE IN BATHROOMS AND LAVARATORIES, 3M TO 4.5M (10 FT TO 15 FT) FROM ANY SWIMMING POOL, DECORATIVE POOLS AND FOUNTAINS, WADING POOLS, CERTAIN THERAPEUTIC POOLS, RESIDENTIAL OUTDOOR USE, TEMPORARY LIGHT AND POWER, CERTAIN HEALTH CARE FACILITIES AREAS, AND STORABLE SWIMMING POOLS. ARROW-HART NO. 1591-F PROTECTS ALL RECEPTACLES DOWNSTREAM

10.	Ground fault interrupter receptacles:

a.	Duplex self protecting type. Similar to No. 1591.

b.	Duplex feed-thru type. Similar to No. 1591-F.

NOTE: - FOR REMOTE CONTROL SWITCH OPERATION.

C.	Momentary Contact Switches:

1.	For remote-control switches: Similar to Pass and Seymour 1251.

D.	Dimmer switches:

1.	Incandescent rotary type.

a.	1000w similar to Pass and Seymour No. 610.

b.	1500w similar to Pass and Seymour No. 615.

c.	2000 w similar to Pass and Seymour No. 620.

NOTE: COORDINATE BALLAST WITH DIMMER SWITCH.

2.	FLUORESCENT ROTARY TYPE.

a.	12-40W LAMPS.

b.	120V AC similar to Pass and Seymour No. -----.

c.	277V AC similar to Pass and Seymour No. -----.

E.	Pilot lights:

1.	Candelabra base receptacle, similar to Arrow-Hart No. 1711.

a.	Rectangular red jewel, similar to Arrow-Hart No. 88.

b.	Round red jewel, similar to Arrow-Hart No. 90.

2.	Neon lamp, 125v AC, similar to Arrow-Hart No. 1720-red.

3.	Neon lamp 220-277v AC, similar to Arrow-Hart No. 1722-red.

NOTE: - COORDINATE FINISH WITH ARCHITECT

F.	Device plates: single plate for multi-switches.

1.	0.04 in. satin finish.

2.	Stainless steel, similar to Arrow-Hart No. 97000 series.

3.	Brass, chrome finish, similar to Arrow-Hart No. 94000 DCH series.

4.	Aluminum, similar to Arrow-Hart No. 95000 series.

5.	Brass brushed finish, similar to Arrow-Hart No. 94000.

6.	For receptacles with other than 120 volt, inscribed voltage available.

7.	Weatherproof outdoor similar to No. 7420-A.

8.	Weatherproof - indoor similar to Pass and Seymour No. 4515.

NOTE: FOR GROUND FAULT CIRCUIT INTERRUPTER RECEPTACLE

9.	Weatherproof cover for standard outlet box, similar to No. 4501.

10.	Weatherproof cover for FS box, similar to No. 4501-FS.

11.	Telephone with 5/8 in. diameter rubber grommeted hole.

NOTE: - ORDINARY PLUG-IN CLOCKS, NON-SYSTEM, WIRED TYPE

G.	Clocks:

1.	Mounting: surface.

2.	Mounting: semi-flush.

3.	12 in. dial.

4.	Black Gothic numerals and sweep second hand.

5.	Similar to: Edwards No. 2215-14 12 in. surface.

6.	Similar to: Edwards No. 2115-14 12 in. semi-flush.

H.	Time switches:

NOTE: FOR INTERIOR LIGHTING

1.	40 amp, 120 volt.

2.	40 amp, 277 volt.

3.	----- pole, ----- throw.

4.	24 hour dial, same ON and OFF time each day.

5.	24 hour dial with skip weekend, same ON and OFF time each day, 1 to 6 day skip feature.

6.	7 day dial, different ON and OFF time each day, skip-day feature.

7.	Intermittent program dial, many ON - OFF times per day, 15 - minute increments.

NOTE: - FOR EXTERIOR LIGHTING.

8.	Astronomical dial, ON at sunset, OFF at sunrise.

9.	Astronomical dial with weekend skip, ON at sunset, OFF at sunrise, skip-day feature.

I.	Plug-in surface metal raceway with devices:

NOTE:MAXIMUM 2 CIRCUITS, 3 NO. 12 WIRES, PREWIRED 15 AMP RECEPTACLES.

1.	Type -----: Maximum 15 amp receptacles, minimum wiring capacity with receptacles: 3 No. 12.

a.	Raceway: 1-9/32 in. high x 3/4 in. deep.

b.	0.04 in. steel base, 0.025 in. snap-in cover.

c.	Receptacles:

(1)	Prewired on 2 alternate circuits.

(2)	15 amp, 125 volt, 2 pole, 3 wire, grounded.

(3)	----- in. on centers.

(4)	Snap-in.

d.	Similar to Wiremold Co., Plugmold No. 2000.

NOTE: -MAXIMUM 6 NO. 12 WIRES, INDIVIDUALLY wIRED 20 AMP RECEPTACLES

2.	Type -----: Maximum 20 amp receptacles, minimum wiring capacity with receptacles: 6 No. 12.

a.	Raceway: 1-1/4 in. high x 7/8 in. deep.

b.	0.04 in. steel base, 0.025 in. snap-in cover.

c.	Receptacles:

(1)	20 amp, 125 volt, 2 pole, 3 wire, grounded.

(2)	----- in. on centers.

(3)	Snap-in.

d.	Similar to Wiremold Co., PlugmoldNo. 2100.

NOTE: -MAXIMUM 10 NO. 12 THROUGH NO. 6 WIRES INDIVIDUALLY WIRED 20 AMP RECEPTACLES OVER 20 AMP SPECIAL OVERSIZE BOX

3.	Type -----: Maximum 20 amp receptacles, except as noted, minimum wiring capacity with receptacles: 10 No. 1.

a.	Raceway: 2-3/4 in. high x 1-7/16 in. deep.

b.	0.04 in. steel base, snap-in cover.

NOTE: - SPECIFY EACH RECEPTACLE IF MORE THAN ONE.

c.	Receptacles:

(1)	----- amp, ----- pole, ----- wire, grounded.

(2)	----- in. on centers.

(3)	Screw-in.

d.	Receptacles over 20 amp: in raceway matching oversize box.

e.	Similar to Wiremold Co., Plugmold No. 3000.

NOTE: CHECK MAXIMUM WIRES, INDIVIDUALLY WIRED 20 AMP THROUGH 60 AMP RECEPTACLES.

4.	[TYPE -----: [MAXIMUM 60 AMP RECEPTACLES.

a.	[RACEWAY: 4-3/4 IN. HIGH X 1-5/8 IN. DEEP.

b.	0.04 IN. STEEL BASE, SNAP-IN COVER.

NOTE: - SPECIFY EACH RECEPTACLE.

c.	Receptacles:

(1)	----- amp, ----- pole, ----- wire, grounded.

(2)	----- in. on centers.

(3)	Screw-in.

d.	Similar to Wiremold Co., Plugmold No. 4000.

NOTE: - CHECK MAXIMUM WIRES, INDIVIDUALLY wIRED 20 AMP THROUGH 60 AMP RECEPTACLES.

5.	TYPE -----: [MAXIMUM 60 AMP RECEPTACLES.

a.	RACEWAY: 4-3/4 IN. HIGH X 3-9/16 IN. DEEP.

b.	0.04 IN. STEEL BASE, SNAP-IN COVER.

NOTE: - SPECIFY EACH RECEPTACLE.

c.	Receptacles:

(1)	----- amp, ----- wire, ----- pole, grounded.

(2)	----- in. on centers.

(3)	Screw-in.

d.	Similar to Wiremold Co., Plugmold No. 6000.

2)	BASE BID MANUFACTURERS

A.	Wall switches, receptacles, device plates and pilot lights

1.	Arrow-Hart.

2.	Bryant.

3.	Circle F.

4.	General Electric.

5.	Hubbell.

6.	Pass and Seymour.

7.	Leviton.

8.	Slater.

B.	Clocks:

1.	Simplex.

2.	Edwards.

3.	Auth.

4.	Honeywell.

5.	Standard Electric Time.

6.	Stromberg Time.

C.	Plug-in surface metal raceways: Wiremold.

D.	Momentary Contact Switches:

1.	Square D.

2.	Cutler-Hammer.

3.	General Electric.

4.	Westinghouse.

E.	Time switches:

1.	Sangamo.

2.	General Electric.

3.	Paragon.

4.	Tork.

F.	Dimmer switches.

1.	Pass and Seymour.

2.	Leviton.

3.	Lutron.

Part 3 -	EXECUTION

1)	INSTALLATION

A.	Suitable outlet box for each or ganged with multi-device plate.

B.	Underplaster reducer for boxes larger than device plate.

C.	Derate dimmer- switches where ganged or separate outlet box for each.

D.	No double banking of dimmer - switches.

E.	Switches on lock-jamb side of door as actually installed.

F.	Cast metal "FS" box for exterior or moist locations.

G.	Device plates:

1.	In moist or exterior locations or where subject to hose washing, weatherproof plates, receptacles GFCI protected.

2.	Plate inscriptions:

a.	Receptacles on emergency supply inscribed, "EMERGENCY SUPPLY".

H.	Each device: minimum rating suited to load and circuit characteristics.

I.	After GFCI breaker or device, maintain separate neutral for each circuit.

J.	Coordinate cutting, obtain pre-cut openings from manufacturer for:

1.	Door switches.

2.	Metal partitions.

3.	Furniture mounted devices.