D06.REV

SIGNAL SYSTEMS FOR HYDRAULIC ELEVATOR WORK

NOTE: MASTER COPY DATE: JULY 27, 1983

Part 1 -	GENERAL

1)	DESCRIPTION

A.	Complete systems of signal equipment and appurtenances:

1.	Car position indicator.

2.	Alarm bell.

3.	Corridor lanterns.

4.	THIS CAR NEXT sign.

5.	Combination position indicator and corridor lantern.

6.	Annunciator.

7.	Traffic Director station.

8.	Hoistway access switches.

9.	Intense Up Peak signs.

10.	Corridor call pushbuttons.

B.	Provide equipment and operation as required, by Code, for the handicapped

2)	SUBMITTALS

A.	Shop drawings:

1.	Submit detailed drawings of all special signal fixtures and cuts of all acceptable standard fixtures

2.	Drawings, cuts: completely dimensioned; indicate faceplate finishes and type of construction in which they will be installed including method of installation

Part 2 -	PRODUCTS

1)	EQUIPMENT AND MATERIAL

A.	Car position indicator:

1.	Electric type.

2.	Install over car entrance.

3.	Plastic floor numerals; shielded light behind each numeral.

4.	Position of car indicated by illumination of corresponding numeral to landing where car is stopped or passing.

5.	Provide "X" indication when elevator travels in express portion of hoistway

6.	Include UP and DOWN indications.

7.	Floor occupancy signs to illuminate simultaneously with respective car button registration.

NOTE: USE 8 FOR NEW YORK CITY PROJECTS ONLY AND ONLY WHEN REQUIRED BY THE OWNER. COORDINATE WITH OWNER AND ARCHITECT

8.	Provide button which shall activate audible floor indicator signal for the handicapped

a.	Locate button in car operating panel in accordance with Code.

b.	Operation of button shall activate audible signal only for desired trip; shall cancel at termination of trip

c.	Design as detailed or directed.

B.	Alarm bells:

NOTE: ONE BELL MAY BE OMITTED IF CAR TRAVEL IS 30 FT - 0 IN. OR LESS

1.	In hoistway pit:

a.	Provide bell in each elevator pit or each combined pit.

b.	Diameter: 6 in. (150mm).

c.	Connect to Alarm pushbutton and EMERGENCY STOP switch in each car operating panel

d.	Include wiring and transformers.

e.	Junction box in each pit for extension by Electrical Contractor.

2.	Under car platforms:

a.	One bell under each car.

b.	Diameter: 6 in. (150mm).

c.	Connect to Alarm pushbutton and EMERGENCY STOP switch in car operating panel

d.	Include wiring and transformers.

C.	Corridor lanterns:

1.	UP and DOWN lanterns at intermediate landings, single lantern at terminal landings

2.	Gongs for each lantern shall sound once for elevator in up direction, twice for elevator in down direction

3.	Illuminate for corresponding direction of car travel and gong sound when elevator is predetermined distance from scheduled floor stop.

4.	Locate as directed.

5.	Design as detailed or directed.

D.	THIS CAR NEXT sign:

1.	Provide THIS CAR NEXT sign over each elevator entrance at first (main) floor in leiu of corridor lantern

2.	Illuminates when corresponding elevator is next to travel in up direction.

3.	Design as detailed or directed.

E.	Combination position indicator and corridor lantern:

1.	Provide fixture combining electric position indicator and landing signal light with gongs

2.	Install over each elevator entrance at first (main) floor.

3.	Position indicator similar to car position indicator specified herein.

4.	Design as detailed or directed.

F.	Annunciator:

1.	UP-DOWN flash light type.

2.	Automatic reset.

3.	Include buzzer to sound momentarily when corridor call is registered.

4.	Provide wiring and transformer.

G.	Traffic Director station:

1.	Provide read out type Traffic Director station for each bank of elevators.

2.	Locate where directed; coordinate with work of other Divisions.

3.	Panel with:

a.	Position and direction indicators for each car.

b.	Corridor call indicator for each direction.

c.	Nonstop indicator for each car.

d.	Elevator intercom master station.

NOTE: COORDINATE "E", "F" AND "G" WITH OTHER TRADES.

e.	[SPACE PROVISIONS FOR TELEPHONE INSTRUMENT.

f.	[FIRE ALARM STATIONS.

g.	[FIRE STRAP KEY.

h.	[SELECTORS FOR OPERATION OF ELEVATORS IN EVENT OF POWER FAILURE.

i.	[SPACE TO RECEIVE ELEVATOR LOBBY IONIZATION DETECTOR ACTIVATION INDICATOR PANEL.

j.	[DESIGN AS DETAILED OR DIRECTED.

H.	[HOISTWAY [ACCESS [SWITCHES:

1.	[TOP LANDING.

2.	[BOTTOM LANDING.

3.	[OPERATION AND EQUIPMENT AS REQUIRED BY [CODE.

I.	[INTENSE [UP-[PEAK [SIGNS:

1.	[PROVIDE AS DETAILED.

2.	[SIGNS TO INDICATE FLOORS; LEGIBLE ONLY WHEN LIT. [SIGNS AUTOMATICALLY LIGHT WHEN [INTENSE [UP-[PEAK IS IN OPERATION

J.	[CORRIDOR [CALL [PUSHBUTTONS:

YPE

YPE

1.	[CALL REGISTER TYPE.

2.	[CALL REGISTER TYPE WITH DIRECTION ARROWS.

YPE

YPE

3.	[TWO BUTTONS AT ALL INTERMEDIATE LANDINGS, SINGLE BUTTON AT EACH TERMINAL LANDING

4.	[ELECTRONIC TOUCH BUTTONS, NOT ACCEPTABLE.

5.	[DESIGN AS DETAILED OR DIRECTED.

Part 3 -	<EXECUTION

1)	FIELD QUALITY CONTROL

A.	Tests

1.	Perform all tests, necessary in opinion of Owner, Authorities having jurisdiction and to satisfy conditions of Contract