D08.REV

CAR EQUIPMENT FOR HYDRAULIC ELEVATOR WORK

NOTE: MASTER COPY DATE: JULY 27, 1983

Part 1 -	GENERAL

1)	DESCRIPTION

A.	Complete car equipment with required appurtenances.

2)	SUBMITTAL

A.	Shop drawings:

1.	Dimensional drawings indicating:

a.	Complete cab details.

b.	Mounting of equipment to car frame.

2.	Renderings of cabs as required.

3)	ALLOWANCES

A.	Passenger cab enclosure:

1.	Allowance:

NOTE: FOR DOMESTIC PROJECTS USE THE FOLLOWING

llow

a.	Include in Base Bid net allowance noted for purchase of elevator cabs, delivered to building

NOTE: FOR FOREIGN PROJECTS USE THE FOLLOWING

b.	Include in Base Bid net allowance noted for purchase of elevator cabs, F.O.B. point of manufacture, ready for export

llow

c.	Allowance shall include:

(1)	Doors.

(2)	Base.

(3)	Wainscoting.

(4)	Entrance columns.

(5)	Transom.

(6)	Ceiling.

(7)	Canopy.

(8)	Top emergency exit.

(9)	Ventilation.

(10)	Lighting.

(11)	Cutouts and reinforcements for attaching mechanical equipment.

(12)	Hinged access door with lock for manual operation, door to match front return panels (only when swing return panels are specified

(13)	Handrails.

(14)	Certificate holder.

(15)	Swing or fixed front return panels.

(16)	Cab as designed and material as selected by Owner.

d.	Allowance shall exclude:

NOTE: FOR DOMESTIC PROJECTS USE THE FOLLOWING:

hanges

(1)	Handling charges by or for Elevator Contractor.

NOTE: FOR FOREIGN PROJECTS USE THE FOLLOWING:

(2)	Handling charges, shipping, insurance and import duties by or for Elevator Contractor

hanges

(3)	Taxes.

(4)	Car door hangers and interlocks.

(5)	Exit lock contacts.

(6)	Platform.

(7)	Car door sill.

(8)	Flooring.

(9)	Operating equipment.

(10)	Installation: cost of installation, part of basic Elevator Work.

NOTE: INCLUDE THE FOLLOWING IN ANY FOREIGN PROJECT:

e.	All costs for shipping from point of manufacture to project site shall be submitted as a separate price with Base Bid. This cost shall be known as the "Elevator Cab Delivery Price"

f.	Owner reserves the right to:

NOTE: FOR DOMESTIC PROJECTS USE:

educt

(1)	Deduct net allowance from elevator contract and purchase cab seprately.

NOTE: FOR FOREIGN PROJECT USE:

(2)	Deduct net allowance and Elevator Cab Delivery Price from elevator and purchase cab separately

educt

(3)	Include cab of a selected manufacturer at a net figure.

B.	Freight cab enclosure:

1.	Allowance: shall include equipment as spcified for passenger cab.

Part 2 -	PRODUCTS

1)	EQUIPMENT AND MATERIAL

A.	Passenger elevator car frame and platform:

1.	Car frame and auxiliary supports.

a.	Structural steel members.

b.	Welded, riveted or bolted to form rigid unit.

2.	Platform:

a.	Designed for Class of loading specified.

b.	Steel frame with steel subfloor or structural steel frame filled with:

ood

(1)	Double wood flooring, each floor minimum 3/4 in. (19 mm) thick marine grade plywood

(2)	Substantial wood or steel stringers and single wood flooring, minimum 3/4 in. (19 mm) thick marine grade plywood

ood

c.	Underside: fireproofed with minimum No. 27 USSG (0.5mm) sheet steel.

d.	Mount on neoprene pads.

e.	Support pads with auxiliary steel, frame, fastened to car frame forming isolated cushion between car and frame

3.	Toe guard:

a.	Minimum No. 16 USSG (1.5mm) cold rolled sheet steel on entrance side.

b.	Full width of entrance.

c.	As required by Code.

4.	Sill:

ype

a.	Extruded aluminum with approved nonslip surface.

b.	Exacast aluminum or approved equal.

c.	Architectural bronze with approved nonslip surface.

ype

d.	Length to accommodate door in fully open position.

e.	Minimum thickness 7/16 in. (11mm).

f.	Grooves machine planed, minimum guide clearance.

g.	Machine rabbeted to receive toe guard.

h.	Securely fastened to platform.

i.	Shimmed to be level.

j.	Parallel to centerline elevator guide rails.

5.	Floor covering:

iles

a.	Rubber tiles:

b.	Vinyl tiles:

c.	Vinyl asbestos tiles:

d.	Rubber tiles with raised disc design:

(1)	3/16 in. (5mm) thick.

(2)	Pattern and color as selected.

(3)	Lay over 1/16 in. (2mm) asphalt felt.

(4)	Cement tile and felt with tile manufacturer's recommended cement.

e.	Tiles and felt by others:

(1)	3/16 in. (5mm) thick.

(2)	Over 1/16 in. (2mm) felt.

(3)	Adjust floor and sill heights accordingly.

f.	Removable carpeting: by others.

iles

B.	Freight elevator car frame and platform:

1.	Car frame and auxiliary supports.

a.	Structural steel members.

b.	Welded, riveted or bolted to form rigid unit.

2.	Platform:

a.	Designed for Class of loading specified.

b.	Structural steel frame and stringers.

c.	Wearing surface:

ood

(1)	Double wood flooring: subfloor 25/32 in. (20mm) pine or fir, top 25/32 in. (20mm) maple.

(2)	Steel flooring: 1/4 in. (6mm) diamond or checkered plate welded or bolted to frame and stringers with support members to prevent bowing

(3)	Aluminum flooring: 1/4 in. (6mm) diamond or checkered plate bolted to frame and stringers with substantial support members to prevent bowing

ood

d.	Underside of wood platforms fireproofed with minimum No. 27 USSG (0.5mm) sheet steel

3.	Toe guard:

a.	Minimum No. 16 USSG (1.5mm) cold rolled sheet steel on entrance side.

b.	Full width of entrance.

c.	Length as required, or to accomodate inching distance.

d.	As required by Code.

4.	Sill:

a.	Nonslip type as approved.

C.	Worklights and receptacles:

1.	On top of car and under platform:

a.	Lamp socket.

b.	Duplex grounded receptacles.

c.	Lamp wire guard.

2.	Provide grounded receptacle in car service panel.

D.	Sidewalk elevator car frame and platform:

1.	Car frame and auxiliary supports:

a.	Structural steel members.

b.	Bow iron.

c.	Welded, riveted or bolted to form rigid unit.

2.	Platform:

a.	Structural steel frame and stringers.

b.	Steel flooring: 1/4 in. (6mm) diamond or checkered plate welded or bolted to frame and stringers with substantial support members to prevent bowing.

3.	Toe guard:

a.	Minimum No. 16 USSG (1.5mm) cold rolled sheet steel on entrance side.

b.	Full width of entrance.

c.	As required by Code.

4.	Sill: nonslip type as approved.

E.	Passenger cab enclosure:

1.	Cab components:

a.	Front wall return panel (stationary or swing out type).

ini

(1)	Minimum 3/4 in. (19mm) plywood with exposed surface of:

elect

(a)	Selected hardwood veneer and finish.

(b)	Selected fruitwood veneer and finish.

(c)	Selected high pressure laminated plastic.

elect

(d)	Back surface: same as exposed face but may be of lower quality, as approved

(e)	Hoistway side: Fireproofed with minimum No. 26 USSG sheet steel.

(2)	Minimum No. 12 B and S gauge (2.7mm) architectural bronze.

(3)	Minimum No. 12 B and S gauge (2.7mm) yellow bronze.

(4)	Minimum No. 14 USSG, (1.9mm), No. 18-8 or No. 302 stainless steel plane surface

(5)	Minimum No. 18 USSG (1.2mm), No. 18-8 or No. 302 rigidized stainless steel pattern as selected with minimum 3/4 in. (19mm) plywood backing

(a)	Hoistway side: Fireproofed with minimum No. 26 USSG sheet steel

(6)	Minimum No. 14 USSG (1.9mm) cold rolled, stretcher leveled furniture steel

ini

b.	Entrance columns:

auge

(1)	Minimum No. 12 B and S gauge (2.7mm) architectural bronze.

(2)	Minimum No. 12 B and S gauge (2.7mm) yellow bronze.

(3)	Minimum No. 14 USSG (1.9mm) stainless steel plane surface.

(4)	Minimum No. 14 USSG (1.9mm) cold rolled, stretcher leveled furniture steel

auge

c.	Side and rear walls:

inimum

(1)	Minimum 3/4 in. (19mm) plywood with exposed surface of:

elect

(a)	Selected hardwood veneer and finish.

(b)	Selected fruitwood veneer and finish.

(c)	Selected high pressure laminated plastic.

elect

(d)	Back surface: same as exposed face, but may be of lower quality. Submit for review

(e)	Hoistway side: Fireproofed with minimum No. 26 USSG sheet steel.

(2)	Minimum No. 12 B and S gauge (2.7mm) architectural bronze.

(3)	Minimum No. 12 B and S gauge (2.7mm) yellow bronze.

(4)	Minimum No. 14 USSG (1.9mm), No. 18-8 or No. 302 stainless steel, plane surface

(5)	Minimum No. 18 USSG (1.2mm), No. 18-8 or No. 302 rigidized stainless steel, pattern as selected, with minimum 3/4 in. (19mm) plywood or approved backing

(a)	Hoisway side: Fireproofed with minimum No. 26 USSG sheet steel.

(6)	Minimum No.14 USSG (1.9mm) cold rolled, stretcher leveled furniture steel

inimum

(7)	Side emergency exit as noted.

(a)	Emergency exit contacts: provide side emergency exit, where required by Code, with electric contacts to prevent operation of car with exit door open. Provide additional "On-Off" switch connected in series with emergency exit contact, as approved, at each emergency side exit opening. Mount on exterior o car enclosure approximately 3 feet (.914m) from the platform level

(8)	Reinforce walls for rigidity and sound deadening.

d.	Removable, decorative panels:

et

(1)	1 set.

(2)	2 sets.

(3)	3 sets.

(4)	4 sets.

et

(5)	Coordinate with side emergency exit.

(6)	Minimum 3/4 in. (19mm) plywood with exposed surface of:

ype

(a)	Selected hardwood veneer and finish.

(b)	Selected fruitwood veneer and finish.

(c)	Selected high pressure laminated plastic.

ype

(d)	Back surface, same material and thickness as face, but may be of lower quality, subject to review.

(7)	Edges: same as face with inconspicuous joints.

(8)	Edges: integral with binding strip on face:

trip

(a)	Binding strip: minimum No. 12 B and S gauge (2.7mm) architectural bronze

(b)	Binding strip: minimum No. 12 B and S gauge (2.7mm) yellow bronze.

(c)	Binding strip: Minimum No. 14 USSG (1.9mm), No. 18-8 or No. 302 stainless steel, plane surface

(d)	Binding strip: metal binder width on face of panel 3/4 in. (19mm) fastenings invisible on face and edge

trip

(9)	Reveals between panels:

ype

(a)	Same as panel face.

(b)	Architectural bronze.

(c)	Yellow bronze.

(d)	No. 18-8 or 302 stainless steel.

(e)	Baked enamel finish, color as selected.

ype

(10)	Panel attached to shell:

(a)	Concealed key slot.

(b)	Readily removable from inside car.

(c)	Secured to prevent rattling.

(d)	Locked in place at top by concealed screws or other positive concealed means

e.	Canopy:

(1)	Minimum No.12 USSG (2.7mm) cold rolled stretcher leveled furniture steel

(2)	Reinforced to support weight of five workmen, minimum as required by Code.

(3)	Sound deadened.

(4)	Top emergency exit, concealed hinges, chain stop, hairline joints, openable from top of car only.

(a)	Interlocked to prevent operation of car with exit door open.

(5)	Provide guard rail at cab top, rear and sides.

f.	Base:

ase

(1)	Cove type with mitered corners.

(2)	Cove type with rounded corners.

(3)	Straight type.

ase

(4)	Height:

ize

(a)	2-1/2 in. (64mm).

(b)	4 in. (102mm).

ize

inish

(5)	Minimum No. 12 B and S gauge (2.7mm) architectural bronze.

(6)	Minimum No. 12 B and S gauge (2.7mm) yellow bronze.

(7)	Minimum No. 14 USSG (1.9mm), No. 18-8 or No. 302 stainless steel, plane surface

(8)	Rubber, color as selected.

(9)	Vinyl, color as selected.

inish

g.	Ventilation:

(1)	Grille of concentric circles in canopy with finish:

ype

(a)	No. 18-8 or No. 302 stainless steel.

(b)	Architectural bronze.

(c)	Yellow bronze.

(d)	Steel painted to match cab side of canopy.

ype

entil

(2)	Inconspicuous ventilation slots: in base on two sides and back.

(3)	Inconspicuous ventilation slots: in side and back walls, above base.

(4)	Ventilation slots: in side and back walls, concealed by removable, decorative panels

entil

ype

(5)	Exhaust type blower on canopy: single speed.

(6)	Exhaust type blower on canopy: two speed.

ype

h.	Handrail:

all

(1)	On back wall.

(2)	On side walls.

(3)	On side and back walls.

all

inish

(4)	No. 18-8 or No. 302 stainless steel.

(5)	Architectural bronze.

(6)	Yellow bronze.

inish

(7)	Approximate section 3/8 in. (9.5mm) x 3 in. (76mm).

(8)	Ends turned back to wall, or as detailed.

(9)	Fastenings: inconspicuous.

(10)	Fastenings shall not protrude from brackets or form rough edges.

(11)	Height above finished cab floor to suit Code requirements for the Handicapped.

i.	Doors:

ide

(1)	Single speed side slide.

(2)	Two speed side slide.

(3)	Single speed center opening.

(4)	Two speed center opening.

ide

(5)	Hollow metal.

(6)	Flush panel.

(7)	Minimum thickness one in. (25mm).

(8)	Formed of minimum No. 16 USSG (1.5mm) cold rolled stretcher leveled furniture steel

(9)	Reinforced full height with formed steel vertical members tying both faces together, maximum 9 in. (229mm) centers.

(10)	Reinforced on inside to receive hangers, guides, leading edge reversing device and door operating equipment.

(11)	Filled with fireproof sound deadening material.

(12)	Two door guides per door.

(a)	Nonmetallic.

(b)	Adjustable.

(c)	Long wearing.

(d)	Minimum clearance in sill groove.

(e)	Quiet in operation.

(13)	Clad door on car side and leading edge with:

auge

(a)	Minimum No. 14 B and S gauge (1.9mm) architectural bronze.

(b)	Minimum No. 14 B and S gauge (1.9mm) yellow bronze.

(c)	Minimum No. 16 USSG (1.5mm) No. 18-8 or No. 302 stainless steel, plane surface

(d)	Selected hardwood veneer and finish.

(e)	Selected fruitwood veneer and finish.

(f)	Selected high pressure laminated plastic.

auge

(g)	Binding strip on top and edges and kick plate on bottom.

ind

(h)	Binding strip: minimum No. 16 USSG (1,5mm), No. 18-8 or No. 302 stainless steel, plane surface

(i)	Binding strip: minimum No. 14 B and S gauge (1.9mm) architectural bronze

(j)	Binding strip: Minimum No. 14 B and S gauge (1.9mm) yellow bronze.

ind

(k)	Binding strip: binder at leading edge shall lap around leading edge.

(l)	Binding strip: 3/4 in. (19mm) wide.

late

(m)	Kick plate: 2-1/2 in. (64mm) high.

(n)	Kick plate: 4 in. (102mm) high.

(o)	Kick plate: 6 in. (152mm) high.

late

(p)	Fastenings: invisible on car side and leading edge.

j.	Lighting and hung ceiling:

(1)	Luminous ceiling type:

(a)	Fluorescent tubes spaced to produce even illumination of suspended diffuser.

(b)	Fluorescent tubes on top exit door within wire mesh enclosure.

(c)	Support diffuser panels on metal framework suspended from canopy, braced to cab walls.

(d)	Frame with minimum 1 in. (25mm) clearance to wall.

rame

(e)	Frame: minimum No. 14 USSG (1.9mm) or equivalent No. 18-8 or No. 302 stainless steel

(f)	Frame: minimum No. 12 B and S gauge (2.7mm) or equivalent architectural bronze

(g)	Frame: minimum No. 12 B and S gauge (2.7mm) or equivalent yellow bronze

rame

iff

(h)	Diffusers: 0.043 in. (1.09mm) in. thick anodized alumimum, egg crate.

(i)	Diffusers: hexagon, honeycomb core, with core totally enclosed with acrylic plastic.

(j)	Diffusers: 1/4 in. (6mm) cells, formed true and symmetrical.

(k)	Diffusers: 1/8 in. (3mm) thick, frosted.

(l)	Diffusers: 1/8 in. (3mm) thick, frosted with prismatic lenses..

(m)	Diffusers: 1/8 in. (3mm) thick, white.

iff

(2)	Trough lighting:

iff

(a)	On two sides.

(b)	On two sides and back.

iff

(c)	Opaque troughs to match finish of respective walls.

(d)	Formed of same material as respective walls.

(e)	Configuration as noted or directed.

(f)	Provide two fluorescent tubes in each trough. Alternate tubes to eliminate end shadows

k.	Pad hooks:

(1)	Provide on front, sides and rear panels:

anels

(a)	Stainless steel.

(b)	Architectural bronze.

(c)	Yellow bronze.

anels

l.	Protection pads:

(1)	Provide for front, sides and rear panels.

(2)	Fitted, quilted, fire retardant canvas.

(3)	Adequately filled to provide proper protection.

(4)	Arrange stitching to prevent sagging.

(5)	Openings, in area of operating and indicating devices, securely finished.

(6)	Heavy duty brass eyelets properly spaced to suit pad hooks.

m.	Certificate holder:

(1)	Frame shall match cab accessory finish.

(2)	Cover, clear plastic.

(3)	Size as required by governing Code.

F.	Freight cab enclosure:

NOTE: COORDINATE CAB HEIGHT WITH DRAWING. MINIMUM 10 FT HIGH INSIDE UNLESS OTHER SPECIAL REQUIREMENTS EXIST

1.	Cab components:

a.	Walls:

(1)	Minimum No. 14 USSG (1.9mm), cold rolled furniture steel.

(2)	Edges of sections bent to form reinforcing and connection flange.

(3)	Provide additional vertical reinforcements to produce rigid wall.

(4)	Provide resilient strip along butting surfaces of joints.

(5)	Joints light tight.

(6)	Reinforced cutouts for button stations, etc.

b.	Entrance columns:

(1)	Minimum No. 14 USSG (1.9mm) cold rolled furniture steel or equivalent.

c.	Canopy:

(1)	Minimum No. 12 USSG (2.7mm), cold rolled furniture steel.

(2)	Reinforced to withstand weight of 5 workmen, minimum as required by Code.

(3)	Hinged section at front, full width of cab, as noted.

(4)	Reinforced openings for lights and ventilator.

(5)	Joints between canopy sections and between canopy and walls shall include resilient strip along butting surfaces

(6)	Joints light tight.

d.	Ventilation:

(1)	Provide two speed exhaust fan in canopy.

e.	Bumpers:

NOTE: INDICATE WALLS ON WHICH BUMPERS SHALL BE MOUNTED.

(1)	[TWO IN. (51MM) X 12 IN. (305MM) NOMINAL SIZE OAK PLANKS ON REAR AND SIDE WALLS.

(2)	[ENDS ROUNDED.

(3)	[BOLTED THROUGH REINFORCEMENTS BEHIND WALL.

(4)	[BOLT HEADS RECESSED BELOW FACE OF PLANK WITH STEEL WASHER UNDER HEAD.

(5)	[CENTERLINE OF BUMPERS 14 IN. (.35M) AND 36 IN. (.91M) ABOVE FINISHED FLOOR

<NOTE: FOR C LOADING USE THE FOLLOWING:

(6)	Provide wainscoating of two in. (51mm) x 12 in. (305mm) oak planks, 6 ft - 0 in. (1.83m) high on rear and side walls

f.	Car gate:

ert

(1)	Vertical rising single unit, steel.

(2)	Vertical rising two section, steel.

ert

(3)	Counterweighted.

(4)	Counterweight guided.

(5)	Vertical steel guide members, rigid, with cross member and diagonal corner braces at top

(6)	Two guides on each side of gate section.

(7)	Gate frame with intermediate members, rigid, as approved.

(8)	Motorized drive unit mounted to vertical guide members.

(9)	Quiet in operation.

(10)	Cable drive between gate and counterweight.

(11)	Gate switch, shall not be operable by hand from within cab.

(12)	Retiring cam, motorized, mounted to vertical guide members.

(13)	Arranged to release interlocks when deenergized.

(14)	Shall not engage interlock release rollers when retracted, energized.

NOTE: USE THE FOLLOWING FOR TWO STOP ELEVATOR.

(15)	Stationary cam arranged to release interlocks.

g.	Lighting:

own

(1)	Provide two downlights, recessed flush.

(2)	Provide four downlights, recessed flush.

(3)	Provide six downlights, recessed flush.

own

(4)	Downlight shall be sized for and provided with 150 watt lamp.

(5)	Downlight equipped with light diffusing shatterproof lens.

(6)	Lamp replaceable from within car.

(7)	Location as noted, for even distribution of light.

h.	Certificate holder:

(1)	Frame shall match cab accessory finish.

(2)	Cover, clear plastic.

(3)	Size as required by governing Code.

2)	ACCEPTABLE MANUFACTURERS

A.	Car equipment:

1.	Armor Elevator Co.

2.	Dover Elevator Co.

3.	Montgomery Elevator Co.

4.	Otis Elevator Co.

5.	Schindler Haughton Elevator Corp.

6.	Westinghouse Elevator Co.

B.	Cab enclosure:

1.	Bostom Metal Door Co.

2.	Globe Van Doorn

3.	Otis Elevator Co.

4.	Parkline Corp.

5.	Tyler Elevator Products.

Part 3 -	EXECUTION

1)	INSTALLATION

A.	Passenger cab enclosure:

1.	Cab components:

a.	Finish:

(1)	Natural metals No. 4 satin finish.

(2)	Cold rolled steel.

(a)	Cleaned and degreased prior to finishing.

(b)	Interior surfaces of closed sections: primed with two coats rust inhibitive primer prior to fabrication

(c)	Exposed exterior surfaces: two coats primer, two coats baked enamel finish in factory

(d)	Exposed surfaces, doors, walls, canopy etc: primed, filled and sanded, reprimed and minimum four coats of baked enamel. Sanded between coats to produce satin smooth finish

(e)	Two colors as approved, ceiling and walls.

(3)	Protect all finished surfaces from damage until ordered by Owner to remove protective material

B.	Freight cab enclosure:

1.	Cab components.

a.	Finish:

(1)	Ferrous metals cleaned and degreased and two coats rust inhibitive primer applied in factory except polished surfaces of gate guide members, etc

(2)	Finish painting, four coats brushed enamel.

(3)	Each coat allowed to dry thoroughly, then sanded and wiped clean before suceeding coat is applied

(4)	Color as approved.

2)	FIELD QUALITY CONTROL.

A.	Tests:

1.	Perform all tests necessary in opinion of Owner, Authorities having jurisdiction and to satisfy conditions of Contract