ELC Des Guide
SECTION  16210
Master - 16210


ELECTRICAL UTILITY SERVICES
Refer to the Construction Documents Directive for general editing procedures and for document coordination procedures.

See the Church Electrical Directives & Guidelines for additional information regarding the work of this Section.

UPDATE  -  1 May 1996

Specify the respective responsibilities of the Contractor and power company in relation to the service entrance clearly in the Project Manual.  Do not show these reponsibilities by note on Drawings.

PART 1 GENERAL
 1.1
SUMMARY
A.
Includes But Not Limited To

Edit paragraph 1 as required for new service or to fit in with an existing service.

1.
Furnish and install service as described in Contract Documents and as required by local serving agency.

2.
Complete cost of service.

B.
Related Sections

1.
Section 16055  -  General Electrical Requirements

PART 2 PRODUCTS  -  Not Used

PART 3 EXECUTION
 3.1
INSTALLATION
A.
Interface With Other Work  -  Coordinate with serving agency on all items, especially service entrance fittings, meter sockets, and current transformer (C/T) boxes where required.
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